5-5 ½ Albion Street Condominium Association
NOI 
 Project Narrative Description supporting documentation

Proposed plan is for the removal and replacement of the existing fieldstone retaining wall

Existing Site Conditions
The subject property consists of a residential lot which is lot number 81 comprised of 5 – 5 ½ 
Existing Resources
Proposed Project

Consultant provides all the necessary information on a stamped/signed plan.  It's pretty simple.  Essentially there is nothing for you to do other than let your consultants provide all the necessary information.  The only thing the con-com is concerned with is the wetland delineation and the work proposed that interacts with the ground which would include any proposed grading.  Property distances from the delineated resource area must be shown on the signed/stamped plan as well as erosion control.
as long specific questions from Con-com are included in the reports & plans from Gordon & Shea's engineers? 
>  The con-com is mostly interested in the location of the wall to the delineated resource based on the Civil Engineer John Judd, Gateway Consultants & Wetland Scientist Evin Guvendiren, DeRosa Environmental Consulting Structural components of the wall are more of an issue for the building inspector.  
Shea plans for the removal & replacement of the retaining wall, deck/stairs & backyard. We are planning to submit all the docs to Amesbury & MA DEP to meet the 7/15 deadline for the 8/5 Amesbury Con-com meeting.
 
Please know how very appreciative we are of your time & expertise give the unfortunate length of time to proceed with the work! 
 
MA DEP & Amesbury require a narrative about the work so any guidance on this is much appreciated.  Thank you again John!
 
· The proposed wall location has a minimum 5 feet offset from the crest of the slope abutting the wetlands. 
· We are in the 50 foot buffer zone now so need to know if this 5 foot offset is correct to meet con-com requirements.  
· Stockwood Excavation will do the work - understand standard silt erosion sediment control fencing 10 foot minimum distance is required at the base of the slope for the construction & the actual wall location is at the discretion of the contractor.
· Wetland slope landscaping will be done for erosion control - plantings for this will need to conform with New England wetlands - i.e. nothing invasive to impact the wetlands -  i.e. Low maintenance Creeping Juniper, Ornamental grasses, Gold Mops, narrow leaf evening primrose
· Conservation Commission Meeting 8/5 6:30 - 8P Zoom meeting - would your or Tyler be able to sit in should they have questions about the Wetland Impact?  We know there will be an additional fee - and greatly appreciate your efforts!  

